VIA INF Driver Release Note

# MS Operating Systems Supported

Windows 95/98/ME, Windows 2000, Windows XP (X86/X64), Windows Server 2003 (X86/x64).

# Release Information

## Release Index:

Version | Release Date
2.80A | 2006/8/29
2.70A | 2005/12/22
2.60A | 2005/11/7
2.50A | 2005/9/14
2.50 | 2005/8/25
2.40B | 2005/4/26
2.40A | 2005/4/20
2.40 | 2005/3/23
2.30C | 2004/11/22
2.21 P1 | 2004/9/24
2.13 | 2004/06/23
2.12 | 2004/06/14
2.11 | 2004/06/04
2.10 P1 | 2004/05/26
2.10 | 2004/04/05
2.00 | 2003/10/27

## Release History:

### 2.80A (U-Setup 5.2.1.15)

Add the following NB Multi-Function IDs into INFs:

; PT900

PCI\VEN_1106&DEV_0340 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_1340 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_2340 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_3340 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_4340 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_5340 ("VIA I/O APIC Interrupt Controller")

PCI\VEN_1106&DEV_6340 ("VIA Security Device")

PCI\VEN_1106&DEV_7340 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_C340 ("VIA PCI to PCI Bridge Controller")

PCI\VEN_1106&DEV_D340 ("VIA PCI to PCI Bridge Controller")

PCI\VEN_1106&DEV_E340 ("VIA PCI to PCI Bridge Controller")

PCI\VEN_1106&DEV_F340 ("VIA PCI to PCI Bridge Controller")

; P4M900

PCI\VEN_1106&DEV_0364 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_1364 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_2364 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_3364 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_4364 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_5364 ("VIA I/O APIC Interrupt Controller")

PCI\VEN_1106&DEV_6364 ("VIA Security Device")

PCI\VEN_1106&DEV_7364 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_A364 ("VIA PCI to PCI Bridge Controller")

PCI\VEN_1106&DEV_C364 ("VIA PCI to PCI Bridge Controller")

### 2.70A (U-Setup 5.2.1.15)

(A) Add the following NB Multi-Function IDs into INFs:

; P4M890

PCI\VEN_1106&DEV_0327 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_1327 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_2327 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_3327 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_4327 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_5327 ("VIA I/O APIC Interrupt Controller")

PCI\VEN_1106&DEV_6327 ("VIA Security Device")

PCI\VEN_1106&DEV_7327 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_A327 ("VIA PCI to PCI Bridge Controller")

PCI\VEN_1106&DEV_C327 ("VIA PCI to PCI Bridge Controller")

(B) Support BIOS separates the PCIE Bridge into different class code.

(C) Fixed a bug which using new BIOS to update PCI to PCIE Bridge driver showing yellow mark from Version 2.60A to Version 2.70A.

### 2.60A (U-Setup 5.2.1.14)

(A) Add the following NB Multi-Function ID into INFs:

; CX700

PCI\VEN_1106&DEV_3324 (“VIA Standard Host Bridge”)

(B) Remove the following IDs into INFs under AMD64 platform.(Installing B198 device driver from AGP driver)

;AGP

PCI\VEN_1106&DEV_B198

(C) Fixed the issue which show English string on Chinese OS under win98se/ME.

##

### 2.50A (U-Setup 5.2.1.13)

(A) Add the cat file for X86 and X64.:

### 2.50 (U-Setup 5.2.1.13)

(A) Add the following NB Multi-Function IDs into INFs:

; CX700

PCI\VEN_1106&DEV_0324 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_1324 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_2324 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_4324 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_7324 (“VIA Standard Host Bridge”)

;VT3351

PCI\VEN_1106&DEV_0351 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_1351 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_2351 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_3351 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_4351 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_5351 ("VIA I/O APIC Interrupt Controller")

PCI\VEN_1106&DEV_7351 (“VIA Standard Host Bridge”)

;K8M890CE

PCI\VEN_1106&DEV_0336 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_1336 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_2336 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_3336 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_4336 (“VIA Standard Host Bridge”)

PCI\VEN_1106&DEV_5336 ("VIA I/O APIC Interrupt Controller")

PCI\VEN_1106&DEV_7336 (“VIA Standard Host Bridge”)

(B) Add the following SB Multi-Function IDs into INFs:

;CX700

PCI\VEN_1106&DEV_8324 ("VIA Standard PCI to ISA Bridge")

PCI\VEN_1106&DEV_324A ("VIA Standard PCI to PCI Bridge")

PCI\VEN_1106&DEV_324B (“VIA Standard Host Bridge")

PCI\VEN_1106&DEV_324E ("VIA Internal Module Bus")

### 2.40B (U-Setup 5.2.1.12)

An external file, Setup.iss, was opened to provide another “auto reboot” option for silent install.

● While the parameter of silent install auto-reboot, /z”reboot” is not present:

● While the BOOTOPTION value is 0, it means the silent installation will not reboot system automatically after executing.

● Once the BOOTOPTION value is 3, it means the silent installation will reboot system automatically after executing.

● While the parameter of silent install auto-reboot, /z”reboot” is present

● Regardless the value of BOOTOPTION to be 0 or 3, U-setup will reboot system automatically after executing.

##

##

### 2.40A (U-Setup 5.2.1.11)

(A) Add the following SB Multi-Function IDs into INFs:

;VT8237A

PCI\VEN_1106&DEV_3337 ("VIA Standard PCI to ISA Bridge")

PCI\VEN_1106&DEV_337A ("VIA Standard PCI to PCI Bridge")

PCI\VEN_1106&DEV_337B ("VIA Standard Host Bridge")

(A) Add the cat file for X86 and X64.:

### 2.40 (U-Setup 5.2.1.11)

(A) Add the following Multi-Function IDs into INFs:

;PT894

PCI\VEN_1106&DEV_0308 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_1308 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_2308 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_4308 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_5308 ("VIA I/O APIC Interrupt Controller")

PCI\VEN_1106&DEV_7308 ("VIA Standard Host Bridge")

; P4M800CE

PCI\VEN_1106&DEV_0314 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_1314 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_2314 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_4314 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_7314 ("VIA Standard Host Bridge")

; P4M800

PCI\VEN_1106&DEV_0296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_1296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_2296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_3296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_4296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_7296 ("VIA Standard Host Bridge")

;K8M890 :

PCI\VEN_1106&DEV_0290 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_1290 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_2290 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_3290 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_4290 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_5290 ("VIA I/O APIC Interrupt Controller")

PCI\VEN_1106&DEV_7290 ("VIA Standard Host Bridge")

(B) Support setup program of AMD64 platform.

(C) Add the following IDs into INFs under AMD64 platform.

;AGP

PCI\VEN_1106&DEV_B198

PCI\VEN_1106&DEV_B188 ("VIA K8 CPU to AGP Controller")

(D) Add the following SB Multi-Function IDs into INFs:

;VT8237A

PCI\VEN_1106&DEV_3337 ("VIA Standard PCI to ISA Bridge")

PCI\VEN_1106&DEV_337A ("VIA Standard PCI to PCI Bridge")

PCI\VEN_1106&DEV_337B ("VIA Standard Host Bridge")

### 2.30C (U-Setup 5.2.1.6)

(A) Add the following Multi-Function IDs into INFs:

PCI\VEN_1106&DEV_0308 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_1308 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_2308 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_3308 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_4308 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_5308 ("VIA I/O APIC Interrupt Controller")

PCI\VEN_1106&DEV_7308 ("VIA Standard Host Bridge")

### 2.21 P1 (U-Setup 5.2.1.6)

(A) Add the following Multi-Function IDs into INFs:

PCI\VEN_1106&DEV_0296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_1296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_2296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_3296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_4296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_7296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_3287 ("VIA Standard PCI to ISA Bridge")

PCI\VEN_1106&DEV_287A ("VIA Standard PCI to PCI Bridge")

PCI\VEN_1106&DEV_287B ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_287C ("VIA Standard PCIE Root Port")

PCI\VEN_1106&DEV_287D ("VIA Standard PCIE Root Port")

PCI\VEN_1106&DEV_287E ("VIA Ultra VLINK Controller")

### 2.13 (U-Setup 5.2.1.2)

(A) Modify the following Multi-Function IDs into INF:

PCI\VEN_1106&DEV_5208.DeviceDesc = "VIA I/O APIC Interrupt Controller"

PCI\VEN_1106&DEV_5238.DeviceDesc = "VIA I/O APIC Interrupt Controller"

(B) Fixed can’t update driver under win98se.

### 2.12 (U-Setup 5.2.1.2)

(A) Add the following Multi-Function IDs into INFs:

PCI\VEN_1106&DEV_A238 ("VIA PCI to PCI Bridge Controller")

PCI\VEN_1106&DEV_C238 ("VIA PCI to PCI Bridge Controller")

PCI\VEN_1106&DEV_D238 ("VIA PCI to PCI Bridge Controller")

PCI\VEN_1106&DEV_E238 ("VIA PCI to PCI Bridge Controller")

PCI\VEN_1106&DEV_F238 ("VIA PCI to PCI Bridge Controller")

### 2.11 (U-Setup 5.2.1.2)

(A) Remove the following Multi-Function IDs into INFs: (Chip not ready)

;P4M800

PCI\VEN_1106&DEV_0296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_1296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_2296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_3296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_4296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_7296 ("VIA Standard Host Bridge")

(B) Remove the following SB Multi-Function IDs into INFs: (Chip not ready)

PCI\VEN_1106&DEV_3287 ("VIA Standard PCI to ISA Bridge")

PCI\VEN_1106&DEV_287A ("VIA Standard PCI to PCI Bridge")

PCI\VEN_1106&DEV_287B ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_287C ("VIA Standard PCIE Root Port")

PCI\VEN_1106&DEV_287D ("VIA Standard PCIE Root Port")

PCI\VEN_1106&DEV_287E ("VIA Ultra VLINK Controller")

### 2.10 P1 (U-Setup 5.2.1.1.1)

(A) Add the following Multi-Function IDs into INFs:

;P4M800

PCI\VEN_1106&DEV_0296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_1296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_2296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_3296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_4296 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_7296 ("VIA Standard Host Bridge")

(B) Add the following SB Multi-Function IDs into INFs:

PCI\VEN_1106&DEV_3287 ("VIA Standard PCI to ISA Bridge")

PCI\VEN_1106&DEV_287A ("VIA Standard PCI to ISA Bridge")

PCI\VEN_1106&DEV_287B ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_287C ("VIA Standard PCIE Root Port")

PCI\VEN_1106&DEV_287D ("VIA Standard PCIE Root Port")

PCI\VEN_1106&DEV_287E ("VIA Ultra VLINK Controller")

(C) Modify the following Multi-Function IDs Section into INFs:

%PCI\VEN_1106&DEV_A208.DeviceDesc% = VIAPCI_DRV, PCI\VEN_1106&DEV_A208

%PCI\VEN_1106&DEV_C208.DeviceDesc% = VIAPCI_DRV, PCI\VEN_1106&DEV_C208

%PCI\VEN_1106&DEV_D208.DeviceDesc% = VIAPCI_DRV, PCI\VEN_1106&DEV_D208

%PCI\VEN_1106&DEV_E208.DeviceDesc% = VIAPCI_DRV, PCI\VEN_1106&DEV_E208

%PCI\VEN_1106&DEV_F208.DeviceDesc% = VIAPCI_DRV, PCI\VEN_1106&DEV_F208

### 2.10

(A) Deleted the following CPU to PCI bridge IDs into INFs:

PCI\VEN_1106&DEV_3102

PCI\VEN_1106&DEV_3103

PCI\VEN_1106&DEV_8235

PCI\VEN_1106&DEV_3158

PCI\VEN_1106&DEV_3158

PCI\VEN_1106&DEV_3202

PCI\VEN_1106&DEV_9238

(B) Deleted the following CPU to AGP bridge IDs into INFs:

PCI\VEN_1106&DEV_b102

PCI\VEN_1106&DEV_b103

PCI\VEN_1106&DEV_b101

PCI\VEN_1106&DEV_b115

PCI\VEN_1106&DEV_b148

PCI\VEN_1106&DEV_b156

PCI\VEN_1106&DEV_b158

PCI\VEN_1106&DEV_b168

PCI\VEN_1106&DEV_b188

PCI\VEN_1106&DEV_b198

PCI\VEN_1106&DEV_8208

(C) Deleted the following Multi-Function IDs into INFs:

;K8T890

PCI\VEN_1106&DEV_A238

PCI\VEN_1106&DEV_C238

PCI\VEN_1106&DEV_D238

PCI\VEN_1106&DEV_E238

PCI\VEN_1106&DEV_F238

(C) Add the following Multi-Function IDs into INFs:

;K8T890

PCI\VEN_1106&DEV_5238 ("VIA I/O APIC Interrupt Controller")

;PT890

PCI\VEN_1106&DEV_0208 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_1208 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_2208 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_4208 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_5208 ("VIA I/O APIC Interrupt Controller")

PCI\VEN_1106&DEV_7208 ("VIA Standard Host Bridge")

(C) Added the following PCI to ISA bridge IDs into INFs:

PCI\VEN_1106&DEV_3287 ("VIA Standard PCI to ISA Bridge")

### 2.00

(A) Deleted the following PCI to ISA bridge IDs into INFs:

PCI\VEN_1106&DEV_3208

PCI\VEN_1106&DEV_3209

(B) Added the following Multi-Function IDs into INFs:

;KT880

PCI\VEN_1106&DEV_0269 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_1269 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_2269 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_3269 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_4269 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_7269 ("VIA Standard Host Bridge")

;

PCI\VEN_1106&DEV_0282 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_1282 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_2282 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_3282 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_4282 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_7282 ("VIA Standard Host Bridge")

;PT890

PCI\VEN_1106&DEV_3208 ("VIA Standard Host Bridge")

PCI\VEN_1106&DEV_A208 ("VIA PCI to PCI Bridge Controller")

PCI\VEN_1106&DEV_C208 ("VIA PCI to PCI Bridge Controller")

PCI\VEN_1106&DEV_D208 ("VIA PCI to PCI Bridge Controller")

PCI\VEN_1106&DEV_E208 ("VIA PCI to PCI Bridge Controller")

PCI\VEN_1106&DEV_F208 ("VIA PCI to PCI Bridge Controller")

(C) Added the following CPU to AGP controller IDs into INFs:

PCI\VEN_1106&DEV_8208