**
**                                                                           
**  VIA Rhine Family Fast Ethernet Adapter
**                                                                           
**  Application note for Windows 2000 RIS server                
**                                                                           
**

Description
============

    Due to this PCI 10/100Mb Ethernet Adapter driver files didn't bundled in 
Windows 2000 Professional Compact Disc, thus we need to add this adapter
manually in order to successfully remote-boot Windows 2000 Professional client.

To Do
=====

    1. Copy following driver files for windows 2000 to I386 folder on the RIS image.
       It should be RemoteInstall\Setup\Language\Images\Dir_name\i386.
       
       copy fetndis.inf RemoteInstall\Setup\Language\Images\Dir_name\i386
       copy fetnd5bv.sys RemoteInstall\Setup\Language\Images\Dir_name\i386
       copy netvt.cat RemoteInstall\Setup\Language\Images\Dir_name\i386
       copy vuins32.dll RemoteInstall\Setup\Language\Images\Dir_name\i386

    2. Create the $oem$ folder at the same level as the \I386 folder of the RIS
       image. For example: 
           RemoteInstall\Setup\%language\Images\%dir_name%\i386
           RemoteInstall\Setup\%language\Images\%dir_name%\$oem$\$1\Drivers\Nic

       Copy the fetndis.inf, fetnd5bv.sys ,netvt.cat and vuins32.dll to this folder($oem$\$1\Drivers\Nic)
 
    3. Make the following changes to the .sif file to be used for this image installation:
        [Unattended]
        OemPreinstall = yes
        OemPnpDriversPath = Drivers\Nic

       NOTE: The default name of the .sif file is 
          RemoteInstall\Setup\Language\Images\Dir_name\I386\Templates\Ristndrd.sif
       NOTE: You can modify the folder name "Drivers\Nic" to other string you want,
             but this folder must be in the \$oem$\$1\. And you also changed the entry
             OemPnPDriversPath = [The folder name you modified]
       
    4. Stop and restart the BINL service on the RIS server. Type the following lines 
       at the command prompt, pressing ENTER after each command: 
        net stop binlsvc
        net start binlsvc
