;Windows 98 WDM Modem Setup File
;Copyright Motorola, Inc. 2003-2006
;Manufacturer: Motorola Inc

[Version]
;This driver is intended for Windows 98 SE only
Signature="$Windows 95$"
Class=WDMMODEM
Provider=%Mfg%
;This driver is digitally signed
CatalogFile = sm5698.cat

[ControlFlags]

[Manufacturer]
%Mfg% = Motorola

[Motorola]
;----------------------------------------------For ECS------------------------------------------------------------------
; AC-Link IDs
%ModemX% = ModemX, PCI\VEN_1039&DEV_7013&SUBSYS_0C051019       ; SiS/ECS

%ModemX% = ModemX, PCI\VEN_1106&DEV_3068&SUBSYS_0C051019       ; VIA/ECS

%ModemX% = ModemX, PCI\VEN_1002&DEV_434D&SUBSYS_0C051019       ; ATI/ECS
%ModemX% = ModemX, PCI\VEN_1002&DEV_436D&SUBSYS_0C051019       ; IXP300/ECS
%ModemX% = ModemX, PCI\VEN_1002&DEV_4378&SUBSYS_0C051019       ; IXP400/ECS
%ModemX% = ModemX, PCI\VEN_1002&DEV_4382&SUBSYS_0C051019       ; IXP600/ECS

%ModemX% = ModemX, PCI\VEN_10DE&DEV_0058&SUBSYS_0C051019       ; nVidia CK804/ECS
%ModemX% = ModemX, PCI\VEN_10DE&DEV_0069&SUBSYS_0C051019       ; nForce2/ECS
%ModemX% = ModemX, PCI\VEN_10DE&DEV_00D9&SUBSYS_0C051019       ; nForce3/ECS
%ModemX% = ModemX, PCI\VEN_10DE&DEV_00E9&SUBSYS_0C051019       ; nForce3+/ECS
%ModemX% = ModemX, PCI\VEN_10DE&DEV_026A&SUBSYS_0C051019       ; nvidia MCP51/ECS

%ModemX% = ModemX, PCI\VEN_8086&DEV_7196&SUBSYS_0C051019       ; Banister
%ModemX% = ModemX, PCI\VEN_8086&DEV_2416&SUBSYS_0C051019       ; Whitney
%ModemX% = ModemX, PCI\VEN_8086&DEV_2426&SUBSYS_0C051019       ; Whitney
%ModemX% = ModemX, PCI\VEN_8086&DEV_2446&SUBSYS_0C051019       ; CNR
%ModemX% = ModemX, PCI\VEN_8086&DEV_2486&SUBSYS_0C051019       ; ICH3 Intel 830 chipset
%ModemX% = ModemX, PCI\VEN_8086&DEV_24C6&SUBSYS_0C051019       ; ICH4
%ModemX% = ModemX, PCI\VEN_8086&DEV_24D6&SUBSYS_0C051019       ; ICH5
%ModemX% = ModemX, PCI\VEN_8086&DEV_25AA&SUBSYS_0C051019  
%ModemX% = ModemX, PCI\VEN_8086&DEV_266D&SUBSYS_0C051019       ; ICH6
%ModemX% = ModemX, PCI\VEN_8086&DEV_27DD&SUBSYS_0C051019       ; ICH7
%ModemX% = ModemX, PCI\VEN_8086&DEV_25A7&SUBSYS_0C051019       ; Hance Rapids ICH 6300ESB

%ModemX% = ModemX, PCI\VEN_10B9&DEV_5457&SUBSYS_0C051019       ; ALi 1535+

;-----------------------------------------------------------------------------------------------------------------------
; PCI
%ModemP% = ModemP, PCI\VEN_1057&DEV_3052&SUBSYS_30341631&REV_04 ; NEC
%ModemP% = ModemP, PCI\VEN_1057&DEV_3052&SUBSYS_30201057&REV_04 ; PCI III (Si3052)
%ModemP% = ModemP, PCI\VEN_1057&DEV_3052&SUBSYS_30001057&REV_04 ; PCI III (Si3052) Mot
%ModemP% = ModemP, PCI\VEN_1057&DEV_3052                        ; PCI III (Si3052) Mot

%ModemP% = ModemP, PCI\VEN_1543&DEV_3052&SUBSYS_30201543&REV_03 ; PCI III (Si3052)
%ModemP% = ModemP, PCI\VEN_1543&DEV_3052&SUBSYS_30001543&REV_03 ; PCI III (Si3052)
%ModemP% = ModemP, PCI\VEN_1543&DEV_3052                        ; M3

; AC-Link
%ModemX% = ModemX, PCI\VEN_8086&DEV_2416&SUBSYS_42508086&REV_02 ; ICH
%ModemX% = ModemX, PCI\VEN_8086&DEV_2416                        ; ICH
%ModemX% = ModemX, PCI\VEN_8086&DEV_2426&SUBSYS_9019107B&REV_02 ; ICH0
%ModemX% = ModemX, PCI\VEN_8086&DEV_2426                        ; ICH0
%ModemX% = ModemX, PCI\VEN_8086&DEV_2446                        ; ICH2
%ModemX% = ModemX, PCI\VEN_8086&DEV_2486                        ; ICH3/MDC (Si3054)
%ModemX% = ModemX, PCI\VEN_8086&DEV_24C6&SUBSYS_4C66134D&REV_02 ; ICH4/MDC
%ModemX% = ModemX, PCI\VEN_8086&DEV_24C6                        ; ICH4
%ModemX% = ModemX, PCI\VEN_8086&DEV_24D6&SUBSYS_80A61043&REV_02 ; ICH5
%ModemX% = ModemX, PCI\VEN_8086&DEV_24D6                        ; ICH5
%ModemX% = ModemX, PCI\VEN_8086&DEV_25A7                        ; Hance Rapids ICH
%ModemX% = ModemX, PCI\VEN_8086&DEV_266D                        ; ICH6
%ModemX% = ModemX, PCI\VEN_8086&DEV_27DD&SUBSYS_19998086&REV_01 ; ICH7
%ModemX% = ModemX, PCI\VEN_8086&DEV_27DD                        ; ICH7
%ModemX% = ModemX, PCI\VEN_8086&DEV_7196                        ; Banister

%ModemX% = ModemX, PCI\VEN_1002&DEV_434D&SUBSYS_81081043&REV_01 ; ATI
%ModemX% = ModemX, PCI\VEN_1002&DEV_434D&SUBSYS_30541057&REV_01 ; ATI
%ModemX% = ModemX, PCI\VEN_1002&DEV_434D                        ; ATI
%ModemX% = ModemX, PCI\VEN_1002&DEV_436D	                    ; IXP300
%ModemX% = ModemX, PCI\VEN_1002&DEV_4378	                    ; IXP400
%ModemX% = ModemX, PCI\VEN_1002&DEV_4382                        ; IXP600

%ModemX% = ModemX, PCI\VEN_1039&DEV_7013&SUBSYS_97391849&REV_A0 ; SIS963L/AMR
%ModemX% = ModemX, PCI\VEN_1039&DEV_7013&SUBSYS_81701509&REV_A0 ; SIS963L
%ModemX% = ModemX, PCI\VEN_1039&DEV_7013&SUBSYS_70131039&REV_A0 ; SIS963L/CNR
%ModemX% = ModemX, PCI\VEN_1039&DEV_7013&SUBSYS_14561043&REV_A0 ;
%ModemX% = ModemX, PCI\VEN_1039&DEV_7013&SUBSYS_02020202&REV_A0 ; SIS/CNR (Si3054)
%ModemX% = ModemX, PCI\VEN_1039&DEV_7013                        ; SIS/CNR (Si3054)

%ModemX% = ModemX, PCI\VEN_10B9&DEV_5457                        ; ALi 1535+

%ModemX% = ModemX, PCI\VEN_10DE&DEV_0058                        ; nVidia CK804
%ModemX% = ModemX, PCI\VEN_10DE&DEV_0069                        ; nForce2/ACR (Si3054)
%ModemX% = ModemX, PCI\VEN_10DE&DEV_00D9                        ; nForce3
%ModemX% = ModemX, PCI\VEN_10DE&DEV_00E9                        ; nForce3+
%ModemX% = ModemX, PCI\VEN_10DE&DEV_026A                        ; nVidia MCP51

%ModemX% = ModemX, PCI\VEN_1106&DEV_3068&SUBSYS_74901462&REV_80 ; VIA8235/CNR 
%ModemX% = ModemX, PCI\VEN_1106&DEV_3068&SUBSYS_4C661543&REV_80 ; VIA8237/CNR
%ModemX% = ModemX, PCI\VEN_1106&DEV_3068&SUBSYS_180613BD&REV_00
%ModemX% = ModemX, PCI\VEN_1106&DEV_3068&SUBSYS_14361043&REV_00 ; L8D VIA
%ModemX% = ModemX, PCI\VEN_1106&DEV_3068                        ; VIA/CNR

[DestinationDirs]
WinSys=10,System32\Drivers
Winld=11
MotICH=10,Motorola\SMSERIAL
MotINF=10,inf\other
MotInstall=10,Motorola\SMSERIAL
MotHelp = 18

[MotICH]
smserial.inf
smserial.sys
motvcd.vxd
sm56.reg
smwdm.inf
Readme.htm
License.htm

[WinSys]
smserial.sys
;This is for overwrite if newer without version dialog; it is ignored if signed packages
ccport.sys,,,0x00000020

[MotInstall]
sm56set.exe
sm56hlpr.exe
sm56unst.exe,,,0x00010000
sm56brz.dll
sm56chs.dll
sm56cht.dll
sm56eng.dll
sm56fra.dll
sm56ger.dll
sm56ita.dll
sm56jpn.dll
sm56esp.dll
sm56dnk.dll
sm56kor.dll

[Winld]
;This is for overwrite if newer without version dialog; it is ignored if signed packages
wdmmdmld.vxd,,,0x00000020

[MotINF]
smserial.inf

[SourceDisksNames]
1="Motorola SM56 Install Disk for Windows 98",,,

[SourceDisksFiles]
ccport.sys = 1
wdmmdmld.vxd = 1
smserial.inf=1
smserial.sys=1
sm56hlpr.exe=1
sm56set.exe=1
motvcd.vxd=1
sm56unst.exe=1
sm56.reg=1
sm56brz.dll =1
sm56chs.dll =1
sm56cht.dll =1
sm56eng.dll =1
sm56fra.dll =1
sm56ger.dll =1
sm56ita.dll =1
sm56jpn.dll =1
sm56esp.dll =1
sm56dnk.dll =1
sm56kor.dll =1
Readme.htm =1
License.htm =1

[Strings]
Mfg = "Motorola Inc"
ModemX="Motorola SM56 WDM Device"
ModemP="Motorola SM56 WDM Device"

[ModemX]
DriverVer=10/09/2006,6.12.04
CopyFiles= WinSys, Winld, MotICH, MotInstall, MotINF
AddReg=ModemX.AddReg, Non_PCI_One

[ModemP]
DriverVer=10/09/2006,6.12.04
CopyFiles= WinSys, Winld, MotICH, MotInstall, MotINF
AddReg=ModemX.AddReg, PCI_One

[ModemX.AddReg]
HKR,,DevLoader,0,*ntkern
HKR,,NTMPDriver,,"smserial.sys,ccport.sys"

[ModemP.AddReg]
HKR,,DevLoader,0,*ntkern
HKR,,NTMPDriver,,"smserial.sys,ccport.sys"

[ModemX.HW]
AddReg=MOTAddReg.HW

[ModemP.HW]
AddReg=MOTAddReg.HW

[MOTAddReg.HW]
HKR,,ChildID,2,"WDM\MOT8888"

[PreCopySection]
HKR,,NoSetupUI,,1

;Options format changed from hexadecimal into decimal
[Non_PCI_One]
HKLM,Software\Motorola\SMSERIAL\Helper\CallProgress, Options,0x00010001,1
HKLM,Software\Motorola\SMSERIAL\Helper\SpeakerPhone, Options,0x00010001,0
HKLM,Software\Motorola\SMSERIAL\Helper\ModemOnHold, Enabled,0x00010001,0
HKLM,Software\Motorola\SMSERIAL\Helper\ModemOnHold, State,0x00010001,2
HKLM,Software\Motorola\SMSERIAL\Helper, Options,0x00010001,49665
HKLM,Software\Motorola\SMSERIAL, CountryCB,0x00010001,1
HKLM,Software\Motorola\SMSERIAL, CCBID,0x00010001,1
HKLM,Software\Motorola\SMSERIAL, EnhancedHWSettings,0x00000001, FF, 7F, 40, 00, FF, 00, 01, 00

[PCI_One]
HKLM,Software\Motorola\SMSERIAL\Helper\CallProgress, Options,0x00010001,1
HKLM,Software\Motorola\SMSERIAL\Helper\SpeakerPhone, Options,0x00010001,0
HKLM,Software\Motorola\SMSERIAL\Helper\ModemOnHold, Enabled,0x00010001,0
HKLM,Software\Motorola\SMSERIAL\Helper\ModemOnHold, State,0x00010001,2
HKLM,Software\Motorola\SMSERIAL\Helper, Options,0x00010001,49665
HKLM,Software\Motorola\SMSERIAL, CountryCB,0x00010001,1
HKLM,Software\Motorola\SMSERIAL, CCBID,0x00010001,1
HKLM,Software\Motorola\SMSERIAL, EnhancedHWSettings,0x00000001, FF, 7F, 40, 00, FF, 00, 01, 00

