;Windows WDM Modem Setup File
;Copyright Motorola, Inc. 2004-2006
;Manufacturer: Motorola Inc

[Version]
Signature      = "$Windows NT$"
Class          = Modem
ClassGUID      = {4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider       = %Mfg%
DriverVer=10/09/2006,6.12.04
;CatalogFile.NT     = sm56nt32.cat
CatalogFile.NTx86   = sm56nt32.cat
CatalogFile.NTamd64 = sm56nt64.cat 

[ControlFlags]

[Manufacturer]
%Mfg% = Motorola,NTx86,NTamd64

[SourceDisksNames]
1=%SM56_DISK_LABEL%,,,\x86

[SourceDisksNames.x86]
1=%SM56_DISK_LABEL%,,,\x86

[SourceDisksNames.amd64]
1=%SM56_DISK_LABEL%,,,\amd64

[SourceDisksFiles]
smserial.sys = 1
sm56.reg     = 1
sm56co6a.dll   = 1
sm56hlpr.exe = 1
sm56brz.dll =1
sm56chs.dll =1
sm56cht.dll =1
sm56eng.dll =1
sm56fra.dll =1
sm56ger.dll =1
sm56ita.dll =1
sm56jpn.dll =1
sm56esp.dll =1
sm56dnk.dll =1
sm56kor.dll =1
Readme.htm =1
License.htm =1

[Motorola]
;----------------------------------------------For ECS------------------------------------------------------------------
; HDAudio IDs
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3026&SUBSYS_0C071019 ; 2nd-gen-ECS

; AC-Link IDs
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013&SUBSYS_0C051019       ; SiS/ECS

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068&SUBSYS_0C051019       ; VIA/ECS

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_434D&SUBSYS_0C051019       ; ATI/ECS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_436D&SUBSYS_0C051019       ; IXP300/ECS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_4378&SUBSYS_0C051019       ; IXP400/ECS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_4382&SUBSYS_0C051019       ; IXP600/ECS

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_0058&SUBSYS_0C051019       ; nVidia CK804/ECS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_0069&SUBSYS_0C051019       ; nForce2/ECS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_00D9&SUBSYS_0C051019       ; nForce3/ECS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_00E9&SUBSYS_0C051019       ; nForce3+/ECS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_026A&SUBSYS_0C051019       ; nVidia MCP51

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_7196&SUBSYS_0C051019       ; Banister
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2416&SUBSYS_0C051019       ; Whitney
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2426&SUBSYS_0C051019       ; Whitney
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2446&SUBSYS_0C051019       ; CNR
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2486&SUBSYS_0C051019       ; ICH3 Intel 830 chipset
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_24C6&SUBSYS_0C051019       ; ICH4
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_24D6&SUBSYS_0C051019       ; ICH5
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_25AA&SUBSYS_0C051019  
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_266D&SUBSYS_0C051019       ; ICH6
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_27DD&SUBSYS_0C051019       ; ICH7
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_25A7&SUBSYS_0C051019       ; Hance Rapids ICH 6300ESB

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10B9&DEV_5457&SUBSYS_0C051019       ; ALi 1535+

;-----------------------------------------------------------------------------------------------------------------------
; HDAudio IDs
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_103C30BF ; HP-TT8 SPUTNIK
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_103C30CB ; HP-AT3 GALAXY
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_103C30CC ; HP-AT5 MARINER
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_152D0761 ; QUANTA-SW7
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_1631C022 ; Asus-T12FJ
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_1631C024 ; Asus-T12MV
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_104310C6 ; Asus
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1543&DEV_3155&SUBSYS_10431336 ; Asus
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_10573055&REV_0701
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_10573355&REV_0701
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_10573055&REV_1007
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_10573255&REV_1007 ; MDC 1.0 Si3054G
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_10573355&REV_1007
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_17C0005E ; ICH7
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3057&SUBSYS_00010001 ; Si3080
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3026&SUBSYS_10573026&REV_1006
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3026&SUBSYS_10573026&REV_0705 ; MDC 1.5 Si3024B 

%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055 ; MDC 1.0 Si3054G
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3057
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3026 ; MDC 1.5 Si3024B 
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1543&DEV_3155 ; M3


; PCI IDs
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1543&DEV_3052&SUBSYS_30001543&REV_03 ; PCI III (Si3052)
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1543&DEV_3052&SUBSYS_30201543&REV_03 ; PCI III (Si3052)
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1543&DEV_3052                        ; PCI III (Si3052) SIL M3

%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1057&DEV_3052&SUBSYS_30001057&REV_04 ; PCI III (Si3052) Mot
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1057&DEV_3052&SUBSYS_30201057&REV_04 ; PCI III (Si3052)
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1057&DEV_3052&SUBSYS_30341631&REV_04 ; PCI III NEC Aztech
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1057&DEV_3052                        ; PCI III (Si3052) MOT

; AC-Link IDs
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_7196                        ; Banister
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2416&SUBSYS_42508086&REV_02 ; Black Pine
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2416                        ; Whitney
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2426&SUBSYS_9019107B&REV_02 ; Black Pine
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2426                        ; Whitney
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2446                        ; CNR
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2486                        ; ICH3 Intel 830 chipset
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_24C6                        ; ICH4
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_24C6&SUBSYS_4C66134D&REV_02 ; ICH4/MDC
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_24D6                        ; ICH5
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_24D6&SUBSYS_80A61043&REV_02 ; ICH5
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_25A7                        ; Hance Rapids ICH 6300ESB
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_266D                        ; ICH6
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_27DD&SUBSYS_19998086&REV_01 ; ICH7
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_27DD                        ; ICH7

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_434D&SUBSYS_81081043&REV_01 ; ATI
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_434D&SUBSYS_30541057&REV_01 ; ATI
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_434D                        ; ATI
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_436D                        ; IXP300
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_4378                        ; IXP400
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_4382                        ; IXP600

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013&SUBSYS_02020202&REV_A0 ; SiS/CNR (Si3054)
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013&SUBSYS_14561043&REV_A0 ; SiS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013&SUBSYS_46031584&REV_A0 ; SiS AVERATEC
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013&SUBSYS_70131039&REV_A0 ; SIS963L/CNR
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013&SUBSYS_97391849&REV_A0 ; SIS963L/AMR
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013&SUBSYS_81701509&REV_A0 ; SIS963L
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013                        ; SiS/CNR (Si3054)

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10B9&DEV_5457                        ; ALi 1535+

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_0058                        ; nVidia CK804
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_0069                        ; nForce2/ACR (Si3054)
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_00D9                        ; nForce3
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_00E9                        ; nForce3+
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_026A                        ; nVidia MCP51

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068&SUBSYS_14361043&REV_00 ; L8D VIA
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068&SUBSYS_180613BD&REV_00
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068&SUBSYS_74901462&REV_80 ; VIA8235/CNR 
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068&SUBSYS_4C661543&REV_80 ; VIA8237/CNR
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068&SUBSYS_101114FF&REV_80 
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068                        ; VIA

[Motorola.NTx86]
;----------------------------------------------For ECS------------------------------------------------------------------
; HDAudio IDs
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3026&SUBSYS_0C071019 ; 2nd-gen-ECS

; AC-Link IDs
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013&SUBSYS_0C051019       ; SiS/ECS

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068&SUBSYS_0C051019       ; VIA/ECS

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_434D&SUBSYS_0C051019       ; ATI/ECS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_436D&SUBSYS_0C051019       ; IXP300/ECS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_4378&SUBSYS_0C051019       ; IXP400/ECS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_4382&SUBSYS_0C051019       ; IXP600/ECS

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_0058&SUBSYS_0C051019       ; nVidia CK804/ECS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_0069&SUBSYS_0C051019       ; nForce2/ECS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_00D9&SUBSYS_0C051019       ; nForce3/ECS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_00E9&SUBSYS_0C051019       ; nForce3+/ECS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_026A&SUBSYS_0C051019       ; nVidia MCP51

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_7196&SUBSYS_0C051019       ; Banister
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2416&SUBSYS_0C051019       ; Whitney
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2426&SUBSYS_0C051019       ; Whitney
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2446&SUBSYS_0C051019       ; CNR
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2486&SUBSYS_0C051019       ; ICH3 Intel 830 chipset
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_24C6&SUBSYS_0C051019       ; ICH4
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_24D6&SUBSYS_0C051019       ; ICH5
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_25AA&SUBSYS_0C051019  
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_266D&SUBSYS_0C051019       ; ICH6
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_27DD&SUBSYS_0C051019       ; ICH7
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_25A7&SUBSYS_0C051019       ; Hance Rapids ICH 6300ESB

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10B9&DEV_5457&SUBSYS_0C051019       ; ALi 1535+

;-----------------------------------------------------------------------------------------------------------------------
; HDAudio IDs

%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_1631C022 ; Asus-T12FJ
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_1631C024 ; Asus-T12MV
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_104310C6 ; Asus
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1543&DEV_3155&SUBSYS_10431336 ; Asus
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_10573055&REV_0701
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_10573355&REV_0701
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_10573055&REV_1007
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_10573255&REV_1007 ; MDC 1.0 Si3054G
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_10573355&REV_1007
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_17C0005E ; ICH7
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3057&SUBSYS_00010001 ; Si3080
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3026&SUBSYS_10573026&REV_1006
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3026&SUBSYS_10573026&REV_0705 ; MDC 1.5 Si3024B 

%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055 ; MDC 1.0 Si3054G
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3057
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3026 ; MDC 1.5 Si3024B 
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1543&DEV_3155 ; M3


; PCI IDs
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1543&DEV_3052&SUBSYS_30001543&REV_03 ; PCI III (Si3052)
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1543&DEV_3052&SUBSYS_30201543&REV_03 ; PCI III (Si3052)
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1543&DEV_3052                        ; PCI III (Si3052) SIL M3

%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1057&DEV_3052&SUBSYS_30001057&REV_04 ; PCI III (Si3052) Mot
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1057&DEV_3052&SUBSYS_30201057&REV_04 ; PCI III (Si3052)
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1057&DEV_3052&SUBSYS_30341631&REV_04 ; PCI III NEC Aztech
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1057&DEV_3052                        ; PCI III (Si3052) MOT

; AC-Link IDs
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_7196                        ; Banister
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2416&SUBSYS_42508086&REV_02 ; Black Pine
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2416                        ; Whitney
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2426&SUBSYS_9019107B&REV_02 ; Black Pine
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2426                        ; Whitney
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2446                        ; CNR
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2486                        ; ICH3 Intel 830 chipset
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_24C6                        ; ICH4
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_24C6&SUBSYS_4C66134D&REV_02 ; ICH4/MDC
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_24D6                        ; ICH5
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_24D6&SUBSYS_80A61043&REV_02 ; ICH5
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_25A7                        ; Hance Rapids ICH 6300ESB
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_266D                        ; ICH6
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_27DD&SUBSYS_19998086&REV_01 ; ICH7
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_27DD                        ; ICH7

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_434D&SUBSYS_81081043&REV_01 ; ATI
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_434D&SUBSYS_30541057&REV_01 ; ATI
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_434D                        ; ATI
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_436D                        ; IXP300
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_4378                        ; IXP400
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_4382                        ; IXP600

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013&SUBSYS_02020202&REV_A0 ; SiS/CNR (Si3054)
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013&SUBSYS_14561043&REV_A0 ; SiS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013&SUBSYS_46031584&REV_A0 ; SiS AVERATEC
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013&SUBSYS_70131039&REV_A0 ; SIS963L/CNR
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013&SUBSYS_97391849&REV_A0 ; SIS963L/AMR
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013&SUBSYS_81701509&REV_A0 ; SIS963L
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013                        ; SiS/CNR (Si3054)

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10B9&DEV_5457                        ; ALi 1535+

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_0058                        ; nVidia CK804
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_0069                        ; nForce2/ACR (Si3054)
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_00D9                        ; nForce3
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_00E9                        ; nForce3+
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_026A                        ; nVidia MCP51

%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068&SUBSYS_14361043&REV_00 ; L8D VIA
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068&SUBSYS_180613BD&REV_00
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068&SUBSYS_74901462&REV_80 ; VIA8235/CNR 
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068&SUBSYS_4C661543&REV_80 ; VIA8237/CNR
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068&SUBSYS_101114FF&REV_80 
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068                        ; VIA

[Motorola.NTamd64]
; HDAudio IDs
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_103C30BF ; HP-TT8 SPUTNIK
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_103C30CB ; HP-AT3 GALAXY
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_103C30CC ; HP-AT5 MARINER
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_152D0761 ; QUANTA-SW7
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_1631C022 ; Asus-T12FJ
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_1631C024 ; Asus-T12MV
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_104310C6 ; Asus
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1543&DEV_3155&SUBSYS_10431336 ; Asus
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_10573055&REV_0701
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_10573355&REV_0701
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_10573055&REV_1007
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_10573255&REV_1007 ; MDC 1.0 Si3054G
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_10573355&REV_1007
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055&SUBSYS_17C0005E          ; ICH7
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3057&SUBSYS_00010001          ; Si3080
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3026&SUBSYS_10573026&REV_1006
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3026&SUBSYS_10573026&REV_0705 ; MDC 1.5 Si3024B 

%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3055 ; MDC 1.0 Si3054G
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3057
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1057&DEV_3026 ; MDC 1.5 Si3024B 
%SM56_HDAUDIO_MODEM_INSTALL% = SM56_HDAUDIO_MODEM_INSTALL, HDAUDIO\FUNC_02&VEN_1543&DEV_3155 ; M3

; PCI IDs
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1543&DEV_3052&SUBSYS_30001543&REV_03 ; PCI III (Si3052)
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1543&DEV_3052&SUBSYS_30201543&REV_03 ; PCI III (Si3052)
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1543&DEV_3052                        ; PCI III (Si3052) SIL M3

%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1057&DEV_3052&SUBSYS_30001057&REV_04 ; PCI III (Si3052) Mot
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1057&DEV_3052&SUBSYS_30201057&REV_04 ; PCI III (Si3052)
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1057&DEV_3052&SUBSYS_30341631&REV_04 ; PCI III NEC Aztech
%SM56_PCI_MODEM_INSTALL% = SM56_PCI_MODEM_INSTALL, PCI\VEN_1057&DEV_3052                        ; PCI III (Si3052) MOT

; AC-Link IDs
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_7196                        ; Banister
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2416                        ; ICH
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2426                        ; ICH0
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2446                        ; ICH2
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_2486                        ; ICH3 Intel 830 chipset
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_24C6                        ; ICH4
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_24D6                        ; ICH5
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_25A7                        ; Hance Rapids ICH 6300ESB
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_266D                        ; ICH6
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_8086&DEV_27DD                        ; ICH7
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_434D                        ; ATI
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_436D                        ; IXP300
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_4378                        ; IXP400
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1002&DEV_4382                        ; IXP600
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013&SUBSYS_46031584&REV_A0 ; SiS AVERATEC
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1039&DEV_7013                        ; SiS
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10B9&DEV_5457                        ; ALi 1535+
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_0058                        ; nVidia CK804
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_0069                        ; nForce2/ACR (Si3054)
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_00D9                        ; nForce3
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_10DE&DEV_026A                        ; nVidia MCP51
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068&SUBSYS_10931734&REV_80 ; VIA
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068&SUBSYS_09011558&REV_80 ; VIA
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068&SUBSYS_101114FF&REV_80 ; VIA
%SM56_MODEM_INSTALL% = SM56_MODEM_INSTALL, PCI\VEN_1106&DEV_3068                        ; VIA



[Strings]
Mfg                        = "Motorola Inc"
SM56_HDAUDIO_MODEM_INSTALL = "Motorola SM56 Data Fax Modem"
SM56_MODEM_INSTALL         = "Motorola SM56 Data Fax Modem"
SM56_PCI_MODEM_INSTALL     = "Motorola SM56 Data Fax Modem"
SM56_DISK_LABEL            = "Motorola SM56 Install Disk for Windows"
ProductName                = "SMSERIAL"

[DestinationDirs]
DefaultDestDirs = 16422,Motorola\%ProductName%
MotSys = 12                            ;winnt\system32\drivers
MotInstall = 16422,Motorola\%ProductName%      ;program files\motorola\smserial
CoInstaller_CopyFiles = 11             ;winnt\system32\
OldMotInstall = 10                             ;old installation
OldDefaultDestDirs = 10,Motorola\%ProductName% ;folders

[OldMotInstall]
sm56itl.dll
sm56spn.dll

[OldDefaultDestDirs]
domestic.chm
brazil.chm
french.chm
german.chm
italian.chm
spanish.chm
Chinese.chm
japanese.chm
korean.chm
dutch.chm
sm56Unst.exe
readme.doc

[DefaultDestDirs]
sm56.reg
Readme.htm
License.htm

[MotInstall]
sm56hlpr.exe
sm56brz.dll
sm56chs.dll
sm56cht.dll
sm56eng.dll
sm56fra.dll
sm56ger.dll
sm56ita.dll
sm56jpn.dll
sm56esp.dll
sm56dnk.dll
sm56kor.dll
 
[MotSys]
smserial.sys

[SM56_HDAUDIO_MODEM_INSTALL.NT]
DriverVer=10/09/2006,6.12.04
CopyFiles = MotInstall, MotSys, DefaultDestDirs
AddReg=All, MfgAddReg, Modem1.AddReg, INTERNAL, Modem1KeyNT, Non_PCI_One, Uninstaller_AddReg
DelReg=Modem_Voice

[SM56_MODEM_INSTALL.NT]
DriverVer=10/09/2006,6.12.04
CopyFiles = MotInstall, MotSys, DefaultDestDirs
AddReg=All, MfgAddReg, Modem1.AddReg, INTERNAL, Modem1KeyNT, Non_PCI_One, Uninstaller_AddReg
DelReg=Modem_Voice

[SM56_PCI_MODEM_INSTALL.NT]
DriverVer=10/09/2006,6.12.04
CopyFiles = MotInstall, MotSys, DefaultDestDirs
AddReg=All, MfgAddReg, Modem1.AddReg, INTERNAL, Modem1KeyNT, PCI_One, Uninstaller_AddReg
DelReg=Modem_Voice

; install drivers as services under
; CCR\services\smxxx
; refers to lower section for details of the service key entry
[SM56_HDAUDIO_MODEM_INSTALL.NT.Services]
AddService=smserial, 0x00000000, smserial_Service_Inst

[SM56_MODEM_INSTALL.NT.Services]
AddService=smserial, 0x00000000, smserial_Service_Inst

[SM56_PCI_MODEM_INSTALL.NT.Services]
AddService=smserial, 0x00000000, smserial_Service_Inst

; adds the lower filter key using addreg section defined below
[SM56_HDAUDIO_MODEM_INSTALL.NT.HW]
AddReg=LowerFilterAddReg

[SM56_MODEM_INSTALL.NT.HW]
AddReg=LowerFilterAddReg

[SM56_PCI_MODEM_INSTALL.NT.HW]
AddReg=LowerFilterAddReg

;-------------- Coinstaller installation
[SM56_HDAUDIO_MODEM_INSTALL.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[SM56_MODEM_INSTALL.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[SM56_PCI_MODEM_INSTALL.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[CoInstaller_CopyFiles]
sm56co6a.dll

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000,"sm56co6a.dll,SM56CoInstaller"

;  add the driver as a lower filter driver under the device key
;  \enum\busenum\devXXXX_venXXXX\<inst id>\lowerfilters REG_MULTIZ
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
[LowerFilterAddReg]
HKR,,"LowerFilters",0x00010000,"smserial"
HKR,,"WakeOnRing",0x00010001,1

;  type=kernel driver  start=manual, pnp will start
[smserial_Service_Inst]
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\smserial.sys

[Uninstaller_AddReg]
HKLM,Software\Microsoft\Windows\CurrentVersion\Uninstall\SMSERIAL,DisplayName,,%SM56_MODEM_INSTALL%
HKLM,Software\Microsoft\Windows\CurrentVersion\Uninstall\SMSERIAL,UninstallString,,"rundll32.exe sm56co6a.dll,SM56UnInstaller"

[Modem1KeyNT]
HKLM,Software\Microsoft\Windows\CurrentVersion\Run,%ProductName%,,%16422%\Motorola\%ProductName%\sm56hlpr.exe
HKLM,Software\Microsoft\Windows\CurrentVersion\RunOnce,%ProductName%,,"rundll32.exe sm56co6a.dll,SM56LaunchHelper"

HKLM,Software\Motorola\SMSERIAL\Helper, SetupFlag,,01
HKLM,Software\Motorola\SMSERIAL\Helper, DriverType,0x00010001,2
HKLM,Software\Motorola\SMSERIAL,QuickConnect1,0x00000001, 00, 00, 03

; The ATI8 command is user definable and is done by updating the string.  There is a
; limit of 50 characters or less.  Add you're string between the "".
HKLM,Software\Motorola\SMSERIAL, ATI8,,""

[Non_PCI_One]
HKLM,Software\Motorola\SMSERIAL\Helper\CallProgress, Options,0x00010001,1
HKLM,Software\Motorola\SMSERIAL\Helper\SpeakerPhone, Options,0x00010001,0
HKLM,Software\Motorola\SMSERIAL\Helper\ModemOnHold, Enabled,0x00010001,0
HKLM,Software\Motorola\SMSERIAL\Helper\ModemOnHold, State,0x00010001,2
HKLM,Software\Motorola\SMSERIAL\Helper, Options,0x00010001,49665
HKLM,Software\Motorola\SMSERIAL, CountryCB,0x00010001,1
HKLM,Software\Motorola\SMSERIAL, CCBID,0x00010001,1
HKLM,Software\Motorola\SMSERIAL, EnhancedHWSettings,0x00000001, FF, 7F, 40, 00, FF, 00, 01, 00
;HKLM,Software\Motorola\SMSERIAL\Tester, SafeMode,0x00010001,0
;HKLM,Software\Motorola\SMSERIAL\Tester, TestingInProgress,0x00010001,0

[PCI_One]
HKLM,Software\Motorola\SMSERIAL\Helper\CallProgress, Options,0x00010001,1
HKLM,Software\Motorola\SMSERIAL\Helper\SpeakerPhone, Options,0x00010001,0
HKLM,Software\Motorola\SMSERIAL\Helper\ModemOnHold, Enabled,0x00010001,0
HKLM,Software\Motorola\SMSERIAL\Helper\ModemOnHold, State,0x00010001,2
HKLM,Software\Motorola\SMSERIAL\Helper, Options,0x00010001,49665
HKLM,Software\Motorola\SMSERIAL, CountryCB,0x00010001,1
HKLM,Software\Motorola\SMSERIAL, CCBID,0x00010001,1
HKLM,Software\Motorola\SMSERIAL, EnhancedHWSettings,0x00000001, FF, 7F, 40, 00, FF, 00, 01, 00
;HKLM,Software\Motorola\SMSERIAL\Tester, SafeMode,0x00010001,0
;HKLM,Software\Motorola\SMSERIAL\Tester, TestingInProgress,0x00010001,0


[Modem1.AddReg]
HKR,, Properties, 1, 80,01,00,00, FF,00,00,00, FF,00,00,00, 07,00,00,00, 0F,00,00,00, 77,03,00,00, 00,C2,01,00, C0,DA,00,00

[All]
HKR,,VUARTPort,,Yes
HKR,,ConfigDialog,,modemui.dll
;HKR,,PortConfigDialog,,modemui.dll
HKR,,FriendlyDriver,,Unimodem.vxd
HKR,,DevLoader,,*vcomm
HKR,,PortSubClass,            1,02
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
HKR, Init,                    1,, "AT<cr>"
HKR, Init,                    2,, "AT&F&D2&C1V1S0=0E0<cr>"
HKR,,WORSettings,0x00010001,0

[Modem_Voice]
HKR,,Enumerator
HKR,, VoiceProfile
HKR, WaveDriver
HKR,, SpeakerPhoneSpecs
HKR, SpeakerPhoneSetVolumeGain
HKR, SpeakerPhoneEnable
HKR, SpeakerPhoneDisable
HKR, SpeakerPhoneMute
HKR, SpeakerPhoneUnMute
HKR, GenerateDigit
HKR, VoiceToDataAnswer
HKR, StartPlay
HKR, StopPlay
HKR, StopPlay
HKR, StartRecord
HKR, StopRecord
HKR,, TerminateRecord
HKR,, TerminatePlay
HKR,, AbortPlay
HKR, LineSetPlayFormat
HKR, LineSetRecordFormat
HKR, VoiceAnswer
HKR, VoiceDialNumberSetup
HKR, EnableCallerID
HKR,, CallerIDPrivate
HKR,, CallerIDOutSide
HKR, EnableDistinctiveRing
HKR,, VariableTerminator


[INTERNAL]
HKR,, DeviceType,             1, 02

[MfgAddReg]
HKR,, InactivityScale,        1, 3c,00,00,00
HKR, Monitor,                 1,, "ATS0=0<cr>"
HKR, Monitor,                 2,, "None"
HKR, Hangup,                  1,, "ATH<cr>"
HKR, Answer,                  1,, "ATA<cr>"
HKR,, Reset,,                 "AT&F<cr>"
HKR, Settings, Prefix,,       "AT"
HKR, Settings, Terminator,,   "<cr>"
HKR, Settings, DialPrefix,,   "D"
HKR, Settings, DialSuffix,,   ";"
HKR, Settings, SpeakerVolume_Low,,   "L0"
HKR, Settings, SpeakerVolume_Med,,   "L2"
HKR, Settings, SpeakerVolume_High,,  "L3"
HKR, Settings, SpeakerMode_Off,,     "M0"
HKR, Settings, SpeakerMode_Dial,,    "M1"
HKR, Settings, SpeakerMode_On,,      "M2"
HKR, Settings, SpeakerMode_Setup,,   "M3"
HKR, Settings, FlowControl_Off,,     "\Q0"
HKR, Settings, FlowControl_Hard,,    "\Q3"
HKR, Settings, FlowControl_Soft,,    "\Q1"
HKR, Settings, ErrorControl_On,,     "\N7"
HKR, Settings, ErrorControl_Off,,    "\N0"
HKR, Settings, ErrorControl_Forced,, "\N6"
HKR, Settings, Compression_On,,      "%%C1"
HKR, Settings, Compression_Off,,     "%%C0"
HKR, Settings, Pulse,,        "P"
HKR, Settings, Tone,,         "T"
HKR, Settings, Blind_Off,,    "X4"
HKR, Settings, Blind_On,,     "X3"
HKR, Settings, CallSetupFailTimer,,  "S7=<#>"
HKR, Settings, InactivityTimeout,,   "\T<#>"
HKR, Settings, Modulation_CCITT,,    "*LS1"
HKR, Settings, Modulation_Bell,,     "*LS0"

HKR, Fax, HardwareFlowControl,, "1"
HKR, Fax, SetupCommand,, "ATS7=60/Q3"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand, 1,,"AT"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand, 2,,"AT&FS0=0E0V1&D2"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand, 3,,"ATL1M1/Q3"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand, 4,,"ATX4"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand, 5,,"AT+FCLASS=1"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand, 6,,"AT+FAA=1"
HKR, Fax\Class1\AdaptiveAnswer\AnswerCommand, 7,,"ATA"
HKR, Fax\Class1\AdaptiveAnswer, ModemResponseFaxDetect,, "FAX"
HKR, Fax\Class1\AdaptiveAnswer, ModemResponseDataConnect,, "CONNECT"
HKR, Fax\Class1\AdaptiveAnswer, ModemResponseDataDetect,, "DATA"
HKR, Fax\Class1\AdaptiveAnswer, ModemResponseFaxConnect,, "CONNECT"

HKR, Responses, "0<cr>",       1, 00, 00, 00,00,00,00, 00,00,00,00 ; OK
HKR, Responses, "1<cr>",       1, 02, 00, 00,00,00,00, 00,00,00,00 ;
HKR, Responses, "2<cr>",       1, 08, 00, 00,00,00,00, 00,00,00,00 ; RING
HKR, Responses, "3<cr>",       1, 04, 00, 00,00,00,00, 00,00,00,00 ; NO CARRIER
HKR, Responses, "4<cr>",       1, 03, 00, 00,00,00,00, 00,00,00,00 ; ERROR
HKR, Responses, "5<cr>",       1, 02, 00, 00,00,00,00, 00,00,00,00 ;
HKR, Responses, "6<cr>",       1, 05, 00, 00,00,00,00, 00,00,00,00 ; NO DIALTONE
HKR, Responses, "7<cr>",       1, 06, 00, 00,00,00,00, 00,00,00,00 ; BUSY
HKR, Responses, "8<cr>",       1, 07, 00, 00,00,00,00, 00,00,00,00 ; NO ANSWER

HKR, Responses, "<cr><lf>OK<cr><lf>",                      1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING<cr><lf>",                    1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>",              1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>",                   1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>",             1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BUSY<cr><lf>",                    1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>",               1, 07, 00, 00,00,00,00, 00,00,00,00
;HKR, Responses, "<cr><lf>FAX<cr><lf>",                     1, 03, 00, 00,00,00,00, 00,00,00,00
;HKR, Responses, "<cr><lf>DATA<cr><lf>",                    1, 03, 00, 00,00,00,00, 00,00,00,00
;HKR, Responses, "<cr><lf>VOICE<cr><lf>",                   1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DELAYED<cr><lf>",                 1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BLACKLISTED<cr><lf>",             1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+FCERROR<cr><lf>",                1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERRM=ICLID_202<cr><lf>",          1, 01, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT<cr><lf>",                 1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT <cr><lf>",                1, 02, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 75<cr><lf>",             1, 02, 00, 4b,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 75/LAPM<cr><lf>",         1, 02, 02, 4b,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 75/MNP<cr><lf>",         1, 02, 02, 4b,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 75/LAPM/V42BIS<cr><lf>",  1, 02, 03, 4b,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 75/LAPM/V44<cr><lf>",  1, 02, 03, 4b,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 75/LAPM/MNP5<cr><lf>",  1, 02, 03, 4b,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 75/MNP/MNP5<cr><lf>",    1, 02, 03, 4b,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 75/MNP/V42BIS<cr><lf>",  1, 02, 03, 4b,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 300<cr><lf>",             1, 02, 00, 2C,01,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 300/LAPM<cr><lf>",         1, 02, 02, 2C,01,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 300/MNP<cr><lf>",         1, 02, 02, 2C,01,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 300/LAPM/V42BIS<cr><lf>",  1, 02, 03, 2C,01,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 300/LAPM/V44<cr><lf>",  1, 02, 03, 2C,01,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 300/LAPM/MNP5<cr><lf>",  1, 02, 03, 2C,01,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 300/MNP/MNP5<cr><lf>",    1, 02, 03, 2C,01,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 300/MNP/V42BIS<cr><lf>",    1, 02, 03, 2C,01,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 600<cr><lf>",             1, 02, 00, 58,02,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 600/LAPM<cr><lf>",         1, 02, 02, 58,02,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 600/MNP<cr><lf>",         1, 02, 02, 58,02,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 600/LAPM/V42BIS<cr><lf>",  1, 02, 03, 58,02,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 600/LAPM/V44<cr><lf>",  1, 02, 03, 58,02,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 600/LAPM/MNP5<cr><lf>",  1, 02, 03, 58,02,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 600/MNP/MNP5<cr><lf>",    1, 02, 03, 58,02,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 600/MNP/V42BIS<cr><lf>",    1, 02, 03, 58,02,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 1200<cr><lf>",            1, 02, 00, B0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1200/LAPM<cr><lf>",        1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1200/MNP<cr><lf>",        1, 02, 02, B0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1200/LAPM/V42BIS<cr><lf>",  1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1200/LAPM/V44<cr><lf>",  1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1200/LAPM/MNP5<cr><lf>",  1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1200/MNP/MNP5<cr><lf>",    1, 02, 03, B0,04,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 1200/MNP/V42BIS<cr><lf>",    1, 02, 03, B0,04,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 2400<cr><lf>",            1, 02, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400/LAPM<cr><lf>",        1, 02, 02, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400/MNP<cr><lf>",        1, 02, 02, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400/LAPM/V42BIS<cr><lf>",  1, 02, 03, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400/LAPM/V44<cr><lf>",  1, 02, 03, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400/LAPM/MNP5<cr><lf>",  1, 02, 03, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400/MNP/MNP5<cr><lf>",    1, 02, 03, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400/MNP/V42BIS<cr><lf>",    1, 02, 03, 60,09,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 4800<cr><lf>",            1, 02, 00, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800/LAPM<cr><lf>",        1, 02, 02, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800/MNP<cr><lf>",        1, 02, 02, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800/LAPM/V42BIS<cr><lf>",  1, 02, 03, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800/LAPM/V44<cr><lf>",  1, 02, 03, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800/LAPM/MNP5<cr><lf>",  1, 02, 03, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800/MNP/MNP5<cr><lf>",    1, 02, 03, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800/MNP/V42BIS<cr><lf>",    1, 02, 03, C0,12,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 7200<cr><lf>",            1, 02, 00, 20,1C,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 7200/LAPM<cr><lf>",        1, 02, 02, 20,1C,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 7200/MNP<cr><lf>",        1, 02, 02, 20,1C,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 7200/LAPM/V42BIS<cr><lf>",  1, 02, 03, 20,1C,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 7200/LAPM/V44<cr><lf>",  1, 02, 03, 20,1C,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 7200/LAPM/MNP5<cr><lf>",  1, 02, 03, 20,1C,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 7200/MNP/MNP5<cr><lf>",    1, 02, 03, 20,1C,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 7200/MNP/V42BIS<cr><lf>",    1, 02, 03, 20,1C,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 9600<cr><lf>",            1, 02, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600/LAPM<cr><lf>",        1, 02, 02, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600/MNP<cr><lf>",        1, 02, 02, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600/LAPM/V42BIS<cr><lf>",  1, 02, 03, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600/LAPM/V44<cr><lf>",  1, 02, 03, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600/LAPM/MNP5<cr><lf>",  1, 02, 03, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600/MNP/MNP5<cr><lf>",    1, 02, 03, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600/MNP/V42BIS<cr><lf>",    1, 02, 03, 80,25,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 12000<cr><lf>",           1, 02, 00, E0,2E,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 12000/LAPM<cr><lf>",       1, 02, 02, E0,2E,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 12000/MNP<cr><lf>",       1, 02, 02, E0,2E,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 12000/LAPM/V42BIS<cr><lf>",  1, 02, 03, E0,2E,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 12000/LAPM/V44<cr><lf>",  1, 02, 03, E0,2E,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 12000/LAPM/MNP5<cr><lf>",  1, 02, 03, E0,2E,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 12000/MNP/MNP5<cr><lf>",    1, 02, 03, E0,2E,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 12000/MNP/V42BIS<cr><lf>",    1, 02, 03, E0,2E,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 14400<cr><lf>",           1, 02, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400/LAPM<cr><lf>",       1, 02, 02, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400/MNP<cr><lf>",       1, 02, 02, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400/LAPM/V42BIS<cr><lf>",  1, 02, 03, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400/LAPM/V44<cr><lf>",  1, 02, 03, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400/LAPM/MNP5<cr><lf>",  1, 02, 03, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400/MNP/MNP5<cr><lf>",    1, 02, 03, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400/MNP/V42BIS<cr><lf>",    1, 02, 03, 40,38,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 16800<cr><lf>",           1, 02, 00, A0,41,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 16800/LAPM<cr><lf>",       1, 02, 02, A0,41,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 16800/MNP<cr><lf>",       1, 02, 02, A0,41,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 16800/LAPM/V42BIS<cr><lf>",  1, 02, 03, A0,41,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 16800/LAPM/V44<cr><lf>",  1, 02, 03, A0,41,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 16800/LAPM/MNP5<cr><lf>",  1, 02, 03, A0,41,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 16800/MNP/MNP5<cr><lf>",    1, 02, 03, A0,41,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 16800/MNP/V42BIS<cr><lf>",    1, 02, 03, A0,41,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 19200<cr><lf>",           1, 02, 00, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200/LAPM<cr><lf>",       1, 02, 02, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200/MNP<cr><lf>",       1, 02, 02, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200/LAPM/V42BIS<cr><lf>",  1, 02, 03, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200/LAPM/V44<cr><lf>",  1, 02, 03, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200/LAPM/MNP5<cr><lf>",  1, 02, 03, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200/MNP/MNP5<cr><lf>",    1, 02, 03, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200/MNP/V42BIS<cr><lf>",    1, 02, 03, 00,4B,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 21600<cr><lf>",           1, 02, 00, 60,54,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 21600/LAPM<cr><lf>",       1, 02, 02, 60,54,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 21600/MNP<cr><lf>",       1, 02, 02, 60,54,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 21600/LAPM/V42BIS<cr><lf>",  1, 02, 03, 60,54,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 21600/LAPM/V44<cr><lf>",  1, 02, 03, 60,54,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 21600/LAPM/MNP5<cr><lf>",  1, 02, 03, 60,54,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 21600/MNP/MNP5<cr><lf>",    1, 02, 03, 60,54,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 21600/MNP/V42BIS<cr><lf>",    1, 02, 03, 60,54,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 24000<cr><lf>",           1, 02, 00, C0,5D,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 24000/LAPM<cr><lf>",       1, 02, 02, C0,5D,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 24000/MNP<cr><lf>",       1, 02, 02, C0,5D,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 24000/LAPM/V42BIS<cr><lf>",  1, 02, 03, C0,5D,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 24000/LAPM/V44<cr><lf>",  1, 02, 03, C0,5D,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 24000/LAPM/MNP5<cr><lf>",  1, 02, 03, C0,5D,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 24000/MNP/MNP5<cr><lf>",    1, 02, 03, C0,5D,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 24000/MNP/V42BIS<cr><lf>",    1, 02, 03, C0,5D,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 26400<cr><lf>",           1, 02, 00, 20,67,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 26400/LAPM<cr><lf>",       1, 02, 02, 20,67,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 26400/MNP<cr><lf>",       1, 02, 02, 20,67,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 26400/LAPM/V42BIS<cr><lf>",  1, 02, 03, 20,67,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 26400/LAPM/V44<cr><lf>",  1, 02, 03, 20,67,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 26400/LAPM/MNP5<cr><lf>",  1, 02, 03, 20,67,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 26400/MNP/MNP5<cr><lf>",    1, 02, 03, 20,67,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 26400/MNP/V42BIS<cr><lf>",    1, 02, 03, 20,67,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 28800<cr><lf>",           1, 02, 00, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800/LAPM<cr><lf>",       1, 02, 02, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800/MNP<cr><lf>",       1, 02, 02, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800/LAPM/V42BIS<cr><lf>",  1, 02, 03, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800/LAPM/V44<cr><lf>",  1, 02, 03, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800/LAPM/MNP5<cr><lf>",  1, 02, 03, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800/MNP/MNP5<cr><lf>",    1, 02, 03, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800/MNP/V42BIS<cr><lf>",    1, 02, 03, 80,70,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 31200<cr><lf>",           1, 02, 00, E0,79,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 31200/LAPM<cr><lf>",       1, 02, 02, E0,79,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 31200/MNP<cr><lf>",       1, 02, 02, E0,79,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 31200/LAPM/V42BIS<cr><lf>",  1, 02, 03, E0,79,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 31200/LAPM/V44<cr><lf>",  1, 02, 03, E0,79,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 31200/LAPM/MNP5<cr><lf>",  1, 02, 03, E0,79,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 31200/MNP/MNP5<cr><lf>",    1, 02, 03, E0,79,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 31200/MNP/V42BIS<cr><lf>",    1, 02, 03, E0,79,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 33600<cr><lf>",           1, 02, 00, 40,83,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33600/LAPM<cr><lf>",       1, 02, 02, 40,83,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33600/MNP<cr><lf>",       1, 02, 02, 40,83,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33600/LAPM/V42BIS<cr><lf>",  1, 02, 03, 40,83,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33600/LAPM/V44<cr><lf>",  1, 02, 03, 40,83,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33600/LAPM/MNP5<cr><lf>",  1, 02, 03, 40,83,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33600/MNP/MNP5<cr><lf>",    1, 02, 03, 40,83,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33600/MNP/V42BIS<cr><lf>",    1, 02, 03, 40,83,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 38400<cr><lf>",           1, 02, 00, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400/LAPM<cr><lf>",       1, 02, 02, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400/MNP<cr><lf>",       1, 02, 02, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400/LAPM/V42BIS<cr><lf>",  1, 02, 03, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400/LAPM/V44<cr><lf>",  1, 02, 03, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400/LAPM/MNP5<cr><lf>",  1, 02, 03, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400/MNP/MNP5<cr><lf>",    1, 02, 03, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400/MNP/V42BIS<cr><lf>",    1, 02, 03, 00,96,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 57600<cr><lf>",           1, 02, 00, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600/LAPM<cr><lf>",       1, 02, 02, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600/MNP<cr><lf>",       1, 02, 02, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600/LAPM/V42BIS<cr><lf>",  1, 02, 03, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600/LAPM/V44<cr><lf>",  1, 02, 03, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600/LAPM/MNP5<cr><lf>",  1, 02, 03, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600/MNP/MNP5<cr><lf>",    1, 02, 03, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600/MNP/V42BIS<cr><lf>",    1, 02, 03, 00,E1,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 115200<cr><lf>",          1, 02, 00, 00,C2,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200/LAPM<cr><lf>",      1, 02, 02, 00,C2,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200/MNP<cr><lf>",      1, 02, 02, 00,C2,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200/LAPM/V42BIS<cr><lf>",  1, 02, 03, 00,C2,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200/LAPM/V44<cr><lf>",  1, 02, 03, 00,C2,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200/LAPM/MNP5<cr><lf>",  1, 02, 03, 00,C2,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200/MNP/MNP5<cr><lf>",    1, 02, 03, 00,C2,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200/MNP/V42BIS<cr><lf>",    1, 02, 03, 00,C2,01,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 32000<cr><lf>",          1, 02, 00, 00,7d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 32000/LAPM<cr><lf>",      1, 02, 02, 00,7d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 32000/MNP<cr><lf>",      1, 02, 02, 00,7d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 32000/LAPM/V42BIS<cr><lf>",  1, 02, 03, 00,7d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 32000/LAPM/V44<cr><lf>",  1, 02, 03, 00,7d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 32000/LAPM/MNP5<cr><lf>",  1, 02, 03, 00,7d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 32000/MNP/MNP5<cr><lf>",    1, 02, 03, 00,7d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 32000/MNP/V42BIS<cr><lf>",    1, 02, 03, 00,7d,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 34000<cr><lf>",          1, 02, 00, d0,84,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34000/LAPM<cr><lf>",      1, 02, 02, d0,84,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34000/MNP<cr><lf>",      1, 02, 02, d0,84,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34000/LAPM/V42BIS<cr><lf>",  1, 02, 03, d0,84,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34000/LAPM/V44<cr><lf>",  1, 02, 03, d0,84,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34000/LAPM/MNP5<cr><lf>",  1, 02, 03, d0,84,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34000/MNP/MNP5<cr><lf>",    1, 02, 03, d0,84,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34000/MNP/V42BIS<cr><lf>",    1, 02, 03, d0,84,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 36000<cr><lf>",          1, 02, 00, a0,8c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 36000/LAPM<cr><lf>",      1, 02, 02, a0,8c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 36000/MNP<cr><lf>",      1, 02, 02, a0,8c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 36000/LAPM/V42BIS<cr><lf>",  1, 02, 03, a0,8c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 36000/LAPM/V44<cr><lf>",  1, 02, 03, a0,8c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 36000/LAPM/MNP5<cr><lf>",  1, 02, 03, a0,8c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 36000/MNP/MNP5<cr><lf>",    1, 02, 03, a0,8c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 36000/MNP/V42BIS<cr><lf>",    1, 02, 03, a0,8c,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 38000<cr><lf>",          1, 02, 00, 70,94,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38000/LAPM<cr><lf>",      1, 02, 02, 70,94,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38000/MNP<cr><lf>",      1, 02, 02, 70,94,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38000/LAPM/V42BIS<cr><lf>",  1, 02, 03, 70,94,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38000/LAPM/V44<cr><lf>",  1, 02, 03, 70,94,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38000/LAPM/MNP5<cr><lf>",  1, 02, 03, 70,94,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38000/MNP/MNP5<cr><lf>",    1, 02, 03, 70,94,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38000/MNP/V42BIS<cr><lf>",    1, 02, 03, 70,94,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 40000<cr><lf>",          1, 02, 00, 40,9c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 40000/LAPM<cr><lf>",      1, 02, 02, 40,9c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 40000/MNP<cr><lf>",      1, 02, 02, 40,9c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 40000/LAPM/V42BIS<cr><lf>",  1, 02, 03, 40,9c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 40000/LAPM/V44<cr><lf>",  1, 02, 03, 40,9c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 40000/LAPM/MNP5<cr><lf>",  1, 02, 03, 40,9c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 40000/MNP/MNP5<cr><lf>",    1, 02, 03, 40,9c,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 40000/MNP/V42BIS<cr><lf>",    1, 02, 03, 40,9c,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 42000<cr><lf>",          1, 02, 00, 10,a4,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42000/LAPM<cr><lf>",      1, 02, 02, 10,a4,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42000/MNP<cr><lf>",      1, 02, 02, 10,a4,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42000/LAPM/V42BIS<cr><lf>",  1, 02, 03, 10,a4,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42000/LAPM/V44<cr><lf>",  1, 02, 03, 10,a4,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42000/LAPM/MNP5<cr><lf>",  1, 02, 03, 10,a4,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42000/MNP/MNP5<cr><lf>",    1, 02, 03, 10,a4,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42000/MNP/V42BIS<cr><lf>",    1, 02, 03, 10,a4,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 44000<cr><lf>",          1, 02, 00, e0,ab,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 44000/LAPM<cr><lf>",      1, 02, 02, e0,ab,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 44000/MNP<cr><lf>",      1, 02, 02, e0,ab,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 44000/LAPM/V42BIS<cr><lf>",  1, 02, 03, e0,ab,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 44000/LAPM/V44<cr><lf>",  1, 02, 03, e0,ab,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 44000/LAPM/MNP5<cr><lf>",  1, 02, 03, e0,ab,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 44000/MNP/MNP5<cr><lf>",    1, 02, 03, e0,ab,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 44000/MNP/V42BIS<cr><lf>",    1, 02, 03, e0,ab,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 46000<cr><lf>",          1, 02, 00, b0,b3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46000/LAPM<cr><lf>",      1, 02, 02, b0,b3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46000/MNP<cr><lf>",      1, 02, 02, b0,b3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46000/LAPM/V42BIS<cr><lf>",  1, 02, 03, b0,b3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46000/LAPM/V44<cr><lf>",  1, 02, 03, b0,b3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46000/LAPM/MNP5<cr><lf>",  1, 02, 03, b0,b3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46000/MNP/MNP5<cr><lf>",    1, 02, 03, b0,b3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46000/MNP/V42BIS<cr><lf>",    1, 02, 03, b0,b3,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 48000<cr><lf>",          1, 02, 00, 80,bb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 48000/LAPM<cr><lf>",      1, 02, 02, 80,bb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 48000/MNP<cr><lf>",      1, 02, 02, 80,bb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 48000/LAPM/V42BIS<cr><lf>",  1, 02, 03, 80,bb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 48000/LAPM/V44<cr><lf>",  1, 02, 03, 80,bb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 48000/LAPM/MNP5<cr><lf>",  1, 02, 03, 80,bb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 48000/MNP/MNP5<cr><lf>",    1, 02, 03, 80,bb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 48000/MNP/V42BIS<cr><lf>",    1, 02, 03, 80,bb,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 50000<cr><lf>",          1, 02, 00, 50,c3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50000/LAPM<cr><lf>",      1, 02, 02, 50,c3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50000/MNP<cr><lf>",      1, 02, 02, 50,c3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50000/LAPM/V42BIS<cr><lf>",  1, 02, 03, 50,c3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50000/LAPM/V44<cr><lf>",  1, 02, 03, 50,c3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50000/LAPM/MNP5<cr><lf>",  1, 02, 03, 50,c3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50000/MNP/MNP5<cr><lf>",    1, 02, 03, 50,c3,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50000/MNP/V42BIS<cr><lf>",    1, 02, 03, 50,c3,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 52000<cr><lf>",          1, 02, 00, 20,cb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 52000/LAPM<cr><lf>",      1, 02, 02, 20,cb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 52000/MNP<cr><lf>",      1, 02, 02, 20,cb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 52000/LAPM/V42BIS<cr><lf>",  1, 02, 03, 20,cb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 52000/LAPM/V44<cr><lf>",  1, 02, 03, 20,cb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 52000/LAPM/MNP5<cr><lf>",  1, 02, 03, 20,cb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 52000/MNP/MNP5<cr><lf>",    1, 02, 03, 20,cb,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 52000/MNP/V42BIS<cr><lf>",    1, 02, 03, 20,cb,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 54000<cr><lf>",          1, 02, 00, f0,d2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54000/LAPM<cr><lf>",      1, 02, 02, f0,d2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54000/MNP<cr><lf>",      1, 02, 02, f0,d2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54000/LAPM/V42BIS<cr><lf>",  1, 02, 03, f0,d2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54000/LAPM/V44<cr><lf>",  1, 02, 03, f0,d2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54000/LAPM/MNP5<cr><lf>",  1, 02, 03, f0,d2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54000/MNP/MNP5<cr><lf>",    1, 02, 03, f0,d2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54000/MNP/V42BIS<cr><lf>",    1, 02, 03, f0,d2,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 56000<cr><lf>",          1, 02, 00, c0,da,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 56000/LAPM<cr><lf>",      1, 02, 02, c0,da,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 56000/MNP<cr><lf>",      1, 02, 02, c0,da,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 56000/LAPM/V42BIS<cr><lf>",  1, 02, 03, c0,da,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 56000/LAPM/V44<cr><lf>",  1, 02, 03, c0,da,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 56000/LAPM/MNP5<cr><lf>",  1, 02, 03, c0,da,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 56000/MNP/MNP5<cr><lf>",    1, 02, 03, c0,da,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 56000/MNP/V42BIS<cr><lf>",    1, 02, 03, c0,da,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 58000<cr><lf>",          1, 02, 00, 90,e2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 58000/LAPM<cr><lf>",      1, 02, 02, 90,e2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 58000/MNP<cr><lf>",      1, 02, 02, 90,e2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 58000/LAPM/V42BIS<cr><lf>",  1, 02, 03, 90,e2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 58000/LAPM/V44<cr><lf>",  1, 02, 03, 90,e2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 58000/LAPM/MNP5<cr><lf>",  1, 02, 03, 90,e2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 58000/MNP/MNP5<cr><lf>",    1, 02, 03, 90,e2,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 58000/MNP/V42BIS<cr><lf>",    1, 02, 03, 90,e2,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 60000<cr><lf>",          1, 02, 00, 60,ea,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 60000/LAPM<cr><lf>",      1, 02, 02, 60,ea,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 60000/MNP<cr><lf>",      1, 02, 02, 60,ea,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 60000/LAPM/V42BIS<cr><lf>",  1, 02, 03, 60,ea,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 60000/LAPM/V44<cr><lf>",  1, 02, 03, 60,ea,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 60000/LAPM/MNP5<cr><lf>",  1, 02, 03, 60,ea,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 60000/MNP/MNP5<cr><lf>",    1, 02, 03, 60,ea,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 60000/MNP/V42BIS<cr><lf>",    1, 02, 03, 60,ea,00,00, 00,00,00,00

; Add the following rates to support V.90
HKR, Responses, "<cr><lf>CONNECT 28000<cr><lf>",          1, 02, 00, 60,6d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28000/LAPM<cr><lf>",      1, 02, 02, 60,6d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28000/MNP<cr><lf>",      1, 02, 02, 60,6d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28000/LAPM/V42BIS<cr><lf>", 1, 02, 03, 60,6d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28000/LAPM/V44<cr><lf>", 1, 02, 03, 60,6d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28000/LAPM/MNP5<cr><lf>", 1, 02, 03, 60,6d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28000/MNP/MNP5<cr><lf>",    1, 02, 03, 60,6d,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28000/MNP/V42BIS<cr><lf>",    1, 02, 03, 60,6d,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 29333<cr><lf>",          1, 02, 00,95,72,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 29333/LAPM<cr><lf>",      1, 02, 02,95,72,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 29333/MNP<cr><lf>",      1, 02, 02, 95,72,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 29333/LAPM/V42BIS<cr><lf>",  1, 02, 03, 95,72,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 29333/LAPM/V44<cr><lf>",  1, 02, 03, 95,72,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 29333/LAPM/MNP5<cr><lf>",  1, 02, 03, 95,72,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 29333/MNP/MNP5<cr><lf>",    1, 02, 03, 95,72,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 29333/MNP/V42BIS<cr><lf>",    1, 02, 03, 95,72,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 30666<cr><lf>",          1, 02, 00, ca,77,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 30666/LAPM<cr><lf>",      1, 02, 02, ca,77,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 30666/MNP<cr><lf>",      1, 02, 02, ca,77,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 30666/LAPM/V42BIS<cr><lf>",  1, 02, 03, ca,77,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 30666/LAPM/V44<cr><lf>",  1, 02, 03, ca,77,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 30666/LAPM/MNP5<cr><lf>",  1, 02, 03, ca,77,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 30666/MNP/MNP5<cr><lf>",    1, 02, 03, ca,77,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 30666/MNP/V42BIS<cr><lf>",    1, 02, 03, ca,77,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 33333<cr><lf>",          1, 02, 00, 35,82,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33333/LAPM<cr><lf>",      1, 02, 02, 35,82,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33333/MNP<cr><lf>",      1, 02, 02, 35,82,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33333/LAPM/V42BIS<cr><lf>",  1, 02, 03, 35,82,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33333/LAPM/V44<cr><lf>",  1, 02, 03, 35,82,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33333/LAPM/MNP5<cr><lf>",  1, 02, 03, 35,82,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33333/MNP/MNP5<cr><lf>",    1, 02, 03, 35,82,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 33333/MNP/V42BIS<cr><lf>",    1, 02, 03, 35,82,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 34666<cr><lf>",          1, 02, 00, 6a,87,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34666/LAPM<cr><lf>",      1, 02, 02, 6a,87,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34666/MNP<cr><lf>",      1, 02, 02, 6a,87,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34666/LAPM/V42BIS<cr><lf>",  1, 02, 03, 6a,87,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34666/LAPM/V44<cr><lf>",  1, 02, 03, 6a,87,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34666/LAPM/MNP5<cr><lf>",  1, 02, 03, 6a,87,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34666/MNP/MNP5<cr><lf>",    1, 02, 03, 6a,87,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 34666/MNP/V42BIS<cr><lf>",    1, 02, 03, 6a,87,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 37333<cr><lf>",          1, 02, 00, d5,91,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 37333/LAPM<cr><lf>",      1, 02, 02, d5,91,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 37333/MNP<cr><lf>",      1, 02, 02, d5,91,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 37333/LAPM/V42BIS<cr><lf>",  1, 02, 03, d5,91,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 37333/LAPM/V44<cr><lf>",  1, 02, 03, d5,91,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 37333/LAPM/MNP5<cr><lf>",  1, 02, 03, d5,91,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 37333/MNP/MNP5<cr><lf>",    1, 02, 03, d5,91,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 37333/MNP/V42BIS<cr><lf>",    1, 02, 03, d5,91,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 38666<cr><lf>",          1, 02, 00, 0a,97,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38666/LAPM<cr><lf>",      1, 02, 02, 0a,97,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38666/MNP<cr><lf>",      1, 02, 02, 0a,97,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38666/LAPM/V42BIS<cr><lf>",  1, 02, 03, 0a,97,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38666/LAPM/V44<cr><lf>",  1, 02, 03, 0a,97,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38666/LAPM/MNP5<cr><lf>",  1, 02, 03, 0a,97,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38666/MNP/MNP5<cr><lf>",    1, 02, 03, 0a,97,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38666/MNP/V42BIS<cr><lf>",    1, 02, 03, 0a,97,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 41333<cr><lf>",          1, 02, 00, 75,a1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 41333/LAPM<cr><lf>",      1, 02, 02, 75,a1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 41333/MNP<cr><lf>",      1, 02, 02, 75,a1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 41333/LAPM/V42BIS<cr><lf>",  1, 02, 03, 75,a1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 41333/LAPM/V44<cr><lf>",  1, 02, 03, 75,a1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 41333/LAPM/MNP5<cr><lf>",  1, 02, 03, 75,a1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 41333/MNP/MNP5<cr><lf>",    1, 02, 03, 75,a1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 41333/MNP/V42BIS<cr><lf>",    1, 02, 03, 75,a1,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 42666<cr><lf>",          1, 02, 00, aa,a6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42666/LAPM<cr><lf>",      1, 02, 02, aa,a6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42666/MNP<cr><lf>",      1, 02, 02, aa,a6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42666/LAPM/V42BIS<cr><lf>",  1, 02, 03, aa,a6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42666/LAPM/V44<cr><lf>",  1, 02, 03, aa,a6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42666/LAPM/MNP5<cr><lf>",  1, 02, 03, aa,a6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42666/MNP/MNP5<cr><lf>",    1, 02, 03, aa,a6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 42666/MNP/V42BIS<cr><lf>",    1, 02, 03, aa,a6,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 45333<cr><lf>",          1, 02, 00, 15,b1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 45333/LAPM<cr><lf>",      1, 02, 02, 15,b1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 45333/MNP<cr><lf>",      1, 02, 02, 15,b1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 45333/LAPM/V42BIS<cr><lf>",  1, 02, 03, 15,b1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 45333/LAPM/V44<cr><lf>",  1, 02, 03, 15,b1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 45333/LAPM/MNP5<cr><lf>",  1, 02, 03, 15,b1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 45333/MNP/MNP5<cr><lf>",    1, 02, 03, 15,b1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 45333/MNP/V42BIS<cr><lf>",    1, 02, 03, 15,b1,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 46666<cr><lf>",          1, 02, 00, 4a,b6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46666/LAPM<cr><lf>",      1, 02, 02, 4a,b6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46666/MNP<cr><lf>",      1, 02, 02, 4a,b6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46666/LAPM/V42BIS<cr><lf>",  1, 02, 03, 4a,b6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46666/LAPM/V44<cr><lf>",  1, 02, 03, 4a,b6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46666/LAPM/MNP5<cr><lf>",  1, 02, 03, 4a,b6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46666/MNP/MNP5<cr><lf>",    1, 02, 03, 4a,b6,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 46666/MNP/V42BIS<cr><lf>",    1, 02, 03, 4a,b6,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 49333<cr><lf>",          1, 02, 00, b5,c0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 49333/LAPM<cr><lf>",      1, 02, 02, b5,c0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 49333/MNP<cr><lf>",      1, 02, 02, b5,c0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 49333/LAPM/V42BIS<cr><lf>",  1, 02, 03, b5,c0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 49333/LAPM/V44<cr><lf>",  1, 02, 03, b5,c0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 49333/LAPM/MNP5<cr><lf>",  1, 02, 03, b5,c0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 49333/MNP/MNP5<cr><lf>",    1, 02, 03, b5,c0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 49333/MNP/V42BIS<cr><lf>",    1, 02, 03, b5,c0,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 50666<cr><lf>",          1, 02, 00, ea,c5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50666/LAPM<cr><lf>",      1, 02, 02, ea,c5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50666/MNP<cr><lf>",      1, 02, 02, ea,c5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50666/LAPM/V42BIS<cr><lf>",  1, 02, 03, ea,c5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50666/LAPM/V44<cr><lf>",  1, 02, 03, ea,c5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50666/LAPM/MNP5<cr><lf>",  1, 02, 03, ea,c5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50666/MNP/MNP5<cr><lf>",    1, 02, 03, ea,c5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 50666/MNP/V42BIS<cr><lf>",    1, 02, 03, ea,c5,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 53333<cr><lf>",          1, 02, 00, 55,d0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 53333/LAPM<cr><lf>",      1, 02, 02, 55,d0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 53333/MNP<cr><lf>",      1, 02, 02, 55,d0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 53333/LAPM/V42BIS<cr><lf>",  1, 02, 03, 55,d0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 53333/LAPM/V44<cr><lf>",  1, 02, 03, 55,d0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 53333/LAPM/MNP5<cr><lf>",  1, 02, 03, 55,d0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 53333/MNP/MNP5<cr><lf>",    1, 02, 03, 55,d0,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 53333/MNP/V42BIS<cr><lf>",    1, 02, 03, 55,d0,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 54666<cr><lf>",          1, 02, 00, 8a,d5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54666/LAPM<cr><lf>",      1, 02, 02, 8a,d5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54666/MNP<cr><lf>",      1, 02, 02, 8a,d5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54666/LAPM/V42BIS<cr><lf>",  1, 02, 03, 8a,d5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54666/LAPM/V44<cr><lf>",  1, 02, 03, 8a,d5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54666/LAPM/MNP5<cr><lf>",  1, 02, 03, 8a,d5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54666/MNP/MNP5<cr><lf>",    1, 02, 03, 8a,d5,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 54666/MNP/V42BIS<cr><lf>",    1, 02, 03, 8a,d5,00,00, 00,00,00,00

